15:47:03.561(dt:0)=>SearchingRegisterFiles - found register file "8858Step000.Register.ovt"; matching to setting file"8858Step000.setting.txt"
15:47:03.577(dt:16)=>decodeTestStepFile - load "8858Step000.setting.txt+8858Step000.Register.ovt.txt" to Zebra
15:47:03.905(dt:0)=>RunRegisterFile() run test step 8858Step000.Register.ovt
15:47:04.514(dt:609)=>getRunStepstate() to get image state
15:47:05.374(dt:860)=>getRunStepstate() - images snapped succeed
15:47:05.374(dt:0)=>GrabImageRequest() - image#0 ~ image#0 raw image with wait
15:47:05.374(dt:0)=>getPicture2Buffer() - start
15:47:05.483(dt:109)=>getPicture2Buffer() - end
15:47:05.499(dt:16)=>getRunStepstate() to get image state
15:47:05.499(dt:0)=>getRunStepstate() - images snapped succeed
15:47:05.499(dt:0)=>GrabImageRequest() - image#1 ~ image#1 raw image with wait
15:47:05.499(dt:0)=>getPicture2Buffer() - start
15:47:05.593(dt:94)=>getPicture2Buffer() - end
15:47:05.608(dt:15)=>getRunStepstate() to get image state
15:47:05.608(dt:0)=>getRunStepstate() - images snapped succeed
15:47:05.608(dt:0)=>GrabImageRequest() - image#2 ~ image#2 raw image with wait
15:47:05.608(dt:0)=>getPicture2Buffer() - start
15:47:05.686(dt:78)=>getPicture2Buffer() - end
15:47:05.733(dt:47)=>getRunStepstate() to get image state
15:47:05.733(dt:0)=>getRunStepstate() - images snapped succeed
15:47:05.733(dt:0)=>GrabImageRequest() - image#3 ~ image#3 raw image with wait
15:47:05.733(dt:0)=>getPicture2Buffer() - start
15:47:05.827(dt:94)=>getPicture2Buffer() - end
15:47:05.858(dt:31)=>getRunStepstate() to get image state
15:47:05.874(dt:16)=>getRunStepstate() - images snapped succeed
15:47:05.874(dt:0)=>GrabImageRequest() - image#4 ~ image#4 raw image with wait
15:47:05.874(dt:0)=>getPicture2Buffer() - start
15:47:05.952(dt:78)=>getPicture2Buffer() - end
15:47:05.968(dt:16)=>getRunStepstate() to get image state
15:47:05.968(dt:0)=>getRunStepstate() - images snapped succeed
15:47:05.968(dt:0)=>GrabImageRequest() - image#5 ~ image#5 raw image with wait
15:47:05.968(dt:0)=>getPicture2Buffer() - start
15:47:06.077(dt:109)=>getPicture2Buffer() - end
15:47:06.108(dt:31)=>getRunStepstate() to get image state
15:47:06.108(dt:0)=>getRunStepstate() - images snapped succeed
15:47:06.108(dt:0)=>GrabImageRequest() - image#6 ~ image#6 raw image with wait
15:47:06.108(dt:0)=>getPicture2Buffer() - start
15:47:06.186(dt:78)=>getPicture2Buffer() - end
15:47:06.202(dt:16)=>getRunStepstate() to get image state
15:47:06.202(dt:0)=>getRunStepstate() - images snapped succeed
15:47:06.202(dt:0)=>GrabImageRequest() - image#7 ~ image#7 raw image with wait
15:47:06.202(dt:0)=>getPicture2Buffer() - start
15:47:06.264(dt:62)=>getPicture2Buffer() - end
15:47:06.280(dt:16)=>getRunStepstate() to get image state
15:47:06.280(dt:0)=>getRunStepstate() - images snapped succeed
15:47:06.280(dt:0)=>GrabImageRequest() - image#8 ~ image#8 raw image with wait
15:47:06.280(dt:0)=>getPicture2Buffer() - start
15:47:06.343(dt:63)=>getPicture2Buffer() - end
15:47:06.358(dt:15)=>getRunStepstate() to get image state
15:47:06.358(dt:0)=>getRunStepstate() - images snapped succeed
15:47:06.358(dt:0)=>GrabImageRequest() - image#9 ~ image#9 raw image with wait
15:47:06.358(dt:0)=>getPicture2Buffer() - start
15:47:06.421(dt:63)=>getPicture2Buffer() - end
15:47:06.436(dt:15)=>getRunStepstate() to get image state
15:47:06.436(dt:0)=>getRunStepstate() - images snapped succeed
15:47:06.436(dt:0)=>GrabImageRequest() - image#10 ~ image#10 raw image with wait
15:47:06.436(dt:0)=>getPicture2Buffer() - start
15:47:06.499(dt:63)=>getPicture2Buffer() - end
15:47:06.514(dt:15)=>getRunStepstate() to get image state
15:47:06.514(dt:0)=>getRunStepstate() - images snapped succeed
15:47:06.514(dt:0)=>GrabImageRequest() - image#11 ~ image#11 raw image with wait
15:47:06.514(dt:0)=>getPicture2Buffer() - start
15:47:06.577(dt:63)=>getPicture2Buffer() - end
15:47:06.593(dt:16)=>getRunStepstate() to get image state
15:47:06.593(dt:0)=>getRunStepstate() - images snapped succeed
15:47:06.593(dt:0)=>GrabImageRequest() - image#12 ~ image#12 raw image with wait
15:47:06.593(dt:0)=>getPicture2Buffer() - start
15:47:06.655(dt:62)=>getPicture2Buffer() - end
15:47:06.671(dt:16)=>getRunStepstate() to get image state
15:47:06.671(dt:0)=>getRunStepstate() - images snapped succeed
15:47:06.671(dt:0)=>GrabImageRequest() - image#13 ~ image#13 raw image with wait
15:47:06.686(dt:15)=>getPicture2Buffer() - start
15:47:06.733(dt:47)=>getPicture2Buffer() - end
15:47:06.749(dt:16)=>getRunStepstate() to get image state
15:47:06.749(dt:0)=>getRunStepstate() - images snapped succeed
15:47:06.749(dt:0)=>GrabImageRequest() - image#14 ~ image#14 raw image with wait
15:47:06.749(dt:0)=>getPicture2Buffer() - start
15:47:06.811(dt:62)=>getPicture2Buffer() - end
15:47:07.030(dt:219)=>getRunStepstate() to get image state
15:47:07.030(dt:0)=>getRunStepstate() - images snapped succeed
15:47:07.030(dt:0)=>GrabImageRequest() - image#15 ~ image#15 raw image with wait
15:47:07.030(dt:0)=>getPicture2Buffer() - start
15:47:07.140(dt:110)=>getPicture2Buffer() - end
15:47:07.171(dt:31)=>getRunStepstate() to get image state
15:47:07.171(dt:0)=>getRunStepstate() - images snapped succeed
15:47:07.171(dt:0)=>GrabImageRequest() - image#16 ~ image#16 raw image with wait
15:47:07.171(dt:0)=>getPicture2Buffer() - start
15:47:07.233(dt:62)=>getPicture2Buffer() - end
15:47:07.249(dt:16)=>getRunStepstate() to get image state
15:47:07.249(dt:0)=>getRunStepstate() - images snapped succeed
15:47:07.249(dt:0)=>GrabImageRequest() - image#17 ~ image#17 raw image with wait
15:47:07.249(dt:0)=>getPicture2Buffer() - start
15:47:07.312(dt:63)=>getPicture2Buffer() - end
15:47:07.437(dt:125)=>getRunStepstate() to get image state
15:47:07.437(dt:0)=>getRunStepstate() - images snapped succeed
15:47:07.437(dt:0)=>GrabImageRequest() - image#18 ~ image#18 raw image with wait
15:47:07.437(dt:0)=>getPicture2Buffer() - start
15:47:07.546(dt:109)=>getPicture2Buffer() - end
15:47:07.593(dt:47)=>getRunStepstate() to get image state
15:47:07.593(dt:0)=>getRunStepstate() - images snapped succeed
15:47:07.593(dt:0)=>GrabImageRequest() - image#19 ~ image#19 raw image with wait
15:47:07.593(dt:0)=>getPicture2Buffer() - start
15:47:07.687(dt:94)=>getPicture2Buffer() - end
15:47:07.687(dt:0)=>getRunStepstate() to get image state
15:47:07.702(dt:15)=>getRunStepstate() - images snapped succeed
15:47:07.702(dt:0)=>GrabImageRequest() - image#20 ~ image#20 raw image with wait
15:47:07.702(dt:0)=>getPicture2Buffer() - start
15:47:07.765(dt:63)=>getPicture2Buffer() - end
15:47:07.765(dt:0)=>getRunStepstate() to get image state
15:47:07.780(dt:15)=>getRunStepstate() - images snapped succeed
15:47:07.780(dt:0)=>GrabImageRequest() - image#21 ~ image#21 raw image with wait
15:47:07.780(dt:0)=>getPicture2Buffer() - start
15:47:07.843(dt:63)=>getPicture2Buffer() - end
15:47:07.858(dt:15)=>getRunStepstate() to get image state
15:47:07.858(dt:0)=>getRunStepstate() - images snapped succeed
15:47:07.858(dt:0)=>GrabImageRequest() - image#22 ~ image#22 raw image with wait
15:47:07.858(dt:0)=>getPicture2Buffer() - start
15:47:07.921(dt:63)=>getPicture2Buffer() - end
15:47:07.952(dt:31)=>getRunStepstate() to get image state
15:47:07.968(dt:16)=>getRunStepstate() - images snapped succeed
15:47:07.968(dt:0)=>GrabImageRequest() - image#23 ~ image#23 raw image with wait
15:47:07.968(dt:0)=>getPicture2Buffer() - start
15:47:08.030(dt:62)=>getPicture2Buffer() - end
15:47:08.030(dt:0)=>getRunStepstate() to get image state
15:47:08.046(dt:16)=>getRunStepstate() - images snapped succeed
15:47:08.046(dt:0)=>GrabImageRequest() - image#24 ~ image#24 raw image with wait
15:47:08.046(dt:0)=>getPicture2Buffer() - start
15:47:08.108(dt:62)=>getPicture2Buffer() - end
15:47:08.124(dt:16)=>getRunStepstate() to get image state
15:47:08.124(dt:0)=>getRunStepstate() - images snapped succeed
15:47:08.124(dt:0)=>GrabImageRequest() - image#0 ~ image#0 raw image with wait
15:47:08.124(dt:0)=>getPicture2Buffer() - start
15:47:08.202(dt:78)=>getPicture2Buffer() - end
15:47:08.202(dt:0)=>getRunStepstate() to get image state
15:47:08.202(dt:0)=>getRunStepstate() - images snapped succeed
15:47:08.202(dt:0)=>GrabImageRequest() - image#1 ~ image#1 raw image with wait
15:47:08.202(dt:0)=>getPicture2Buffer() - start
15:47:08.280(dt:78)=>getPicture2Buffer() - end
15:47:08.796(dt:516)=>getRunStepstate() to get image state
15:47:08.796(dt:0)=>getRunStepstate() - images snapped succeed
15:47:08.796(dt:0)=>GrabImageRequest() - image#2 ~ image#2 raw image with wait
15:47:08.796(dt:0)=>getPicture2Buffer() - start
15:47:08.874(dt:78)=>getPicture2Buffer() - end
15:47:08.890(dt:16)=>getRunStepstate() to get image state
15:47:08.890(dt:0)=>getRunStepstate() - images snapped succeed
15:47:08.890(dt:0)=>GrabImageRequest() - image#3 ~ image#3 raw image with wait
15:47:08.890(dt:0)=>getPicture2Buffer() - start
15:47:08.952(dt:62)=>getPicture2Buffer() - end
15:47:08.968(dt:16)=>getRunStepstate() to get image state
15:47:08.983(dt:15)=>getRunStepstate() - images snapped succeed
15:47:08.983(dt:0)=>GrabImageRequest() - image#4 ~ image#4 raw image with wait
15:47:08.983(dt:0)=>getPicture2Buffer() - start
15:47:09.046(dt:63)=>getPicture2Buffer() - end
15:47:09.124(dt:78)=>getRunStepstate() to get image state
15:47:09.124(dt:0)=>getRunStepstate() - images snapped succeed
15:47:09.124(dt:0)=>GrabImageRequest() - image#5 ~ image#5 raw image with wait
15:47:09.124(dt:0)=>getPicture2Buffer() - start
15:47:09.187(dt:63)=>getPicture2Buffer() - end
16:00:47.978(dt:0)=>SearchingRegisterFiles - found register file "8858Step000.Register.ovt"; matching to setting file"8858Step000.setting.txt"
16:00:47.994(dt:16)=>decodeTestStepFile - load "8858Step000.setting.txt+8858Step000.Register.ovt.txt" to Zebra
16:00:49.666(dt:0)=>RunRegisterFile() run test step 8858Step000.Register.ovt
16:00:50.291(dt:625)=>getRunStepstate() to get image state
16:00:51.151(dt:860)=>getRunStepstate() - images snapped succeed
16:00:51.151(dt:0)=>GrabImageRequest() - image#0 ~ image#0 raw image with wait
16:00:51.151(dt:0)=>getPicture2Buffer() - start
16:00:51.213(dt:62)=>getPicture2Buffer() - end
16:00:54.870(dt:3657)=>getRunStepstate() to get image state
16:00:54.870(dt:0)=>getRunStepstate() - images snapped succeed
16:00:54.870(dt:0)=>GrabImageRequest() - image#1 ~ image#1 raw image with wait
16:00:54.870(dt:0)=>getPicture2Buffer() - start
16:00:54.932(dt:62)=>getPicture2Buffer() - end
16:00:57.729(dt:2797)=>getRunStepstate() to get image state
16:00:57.729(dt:0)=>getRunStepstate() - images snapped succeed
16:00:57.729(dt:0)=>GrabImageRequest() - image#2 ~ image#2 raw image with wait
16:00:57.729(dt:0)=>getPicture2Buffer() - start
16:00:57.792(dt:63)=>getPicture2Buffer() - end
16:01:01.495(dt:3703)=>getRunStepstate() to get image state
16:01:01.495(dt:0)=>getRunStepstate() - images snapped succeed
16:01:01.495(dt:0)=>GrabImageRequest() - image#3 ~ image#3 raw image with wait
16:01:01.495(dt:0)=>getPicture2Buffer() - start
16:01:01.558(dt:63)=>getPicture2Buffer() - end
16:01:03.948(dt:2390)=>getRunStepstate() to get image state
16:01:03.964(dt:16)=>getRunStepstate() - images snapped succeed
16:01:03.964(dt:0)=>GrabImageRequest() - image#4 ~ image#4 raw image with wait
16:01:03.964(dt:0)=>getPicture2Buffer() - start
16:01:04.026(dt:62)=>getPicture2Buffer() - end
16:01:06.917(dt:2891)=>getRunStepstate() to get image state
16:01:06.917(dt:0)=>getRunStepstate() - images snapped succeed
16:01:06.917(dt:0)=>GrabImageRequest() - image#5 ~ image#5 raw image with wait
16:01:06.917(dt:0)=>getPicture2Buffer() - start
16:01:06.995(dt:78)=>getPicture2Buffer() - end
16:01:10.605(dt:3610)=>getRunStepstate() to get image state
16:01:10.605(dt:0)=>getRunStepstate() - images snapped succeed
16:01:10.605(dt:0)=>GrabImageRequest() - image#6 ~ image#6 raw image with wait
16:01:10.605(dt:0)=>getPicture2Buffer() - start
16:01:10.667(dt:62)=>getPicture2Buffer() - end
16:01:13.480(dt:2813)=>getRunStepstate() to get image state
16:01:13.480(dt:0)=>getRunStepstate() - images snapped succeed
16:01:13.480(dt:0)=>GrabImageRequest() - image#7 ~ image#7 raw image with wait
16:01:13.480(dt:0)=>getPicture2Buffer() - start
16:01:13.558(dt:78)=>getPicture2Buffer() - end
16:01:15.965(dt:2407)=>getRunStepstate() to get image state
16:01:15.965(dt:0)=>getRunStepstate() - images snapped succeed
16:01:15.981(dt:16)=>GrabImageRequest() - image#8 ~ image#8 raw image with wait
16:01:15.981(dt:0)=>getPicture2Buffer() - start
16:01:16.043(dt:62)=>getPicture2Buffer() - end
16:01:19.684(dt:3641)=>getRunStepstate() to get image state
16:01:19.684(dt:0)=>getRunStepstate() - images snapped succeed
16:01:19.684(dt:0)=>GrabImageRequest() - image#9 ~ image#9 raw image with wait
16:01:19.684(dt:0)=>getPicture2Buffer() - start
16:01:19.746(dt:62)=>getPicture2Buffer() - end
16:01:22.497(dt:2751)=>getRunStepstate() to get image state
16:01:22.512(dt:15)=>getRunStepstate() - images snapped succeed
16:01:22.512(dt:0)=>GrabImageRequest() - image#10 ~ image#10 raw image with wait
16:01:22.512(dt:0)=>getPicture2Buffer() - start
16:01:22.575(dt:63)=>getPicture2Buffer() - end
16:01:25.387(dt:2812)=>getRunStepstate() to get image state
16:01:25.387(dt:0)=>getRunStepstate() - images snapped succeed
16:01:25.387(dt:0)=>GrabImageRequest() - image#11 ~ image#11 raw image with wait
16:01:25.387(dt:0)=>getPicture2Buffer() - start
16:01:25.450(dt:63)=>getPicture2Buffer() - end
16:01:28.716(dt:3266)=>getRunStepstate() to get image state
16:01:28.716(dt:0)=>getRunStepstate() - images snapped succeed
16:01:28.716(dt:0)=>GrabImageRequest() - image#12 ~ image#12 raw image with wait
16:01:28.716(dt:0)=>getPicture2Buffer() - start
16:01:28.794(dt:78)=>getPicture2Buffer() - end
16:01:54.860(dt:0)=>SearchingRegisterFiles - found register file "8858Step000.Register.ovt"; matching to setting file"8858Step000.setting.txt"
16:01:54.860(dt:0)=>decodeTestStepFile - load "8858Step000.setting.txt+8858Step000.Register.ovt.txt" to Zebra
